--  =================================================================
-- Copyright (C) 2015 by HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: Huawei NETSTREAM MIB File for environment
-- Reference:   
-- Version:     V2.01
-- History:
-- 
--  2005-10-26  V1.00   Zhang Xiaomeng(ht09867), Initial Version 
--  2015-08-01  V2.00   d00296290
--  2015-08-06  V2.01   d00296290, add node for template refresh
-- =================================================================

HUAWEI-NETSTREAM-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        hwDatacomm
            FROM HUAWEI-MIB
        MODULE-COMPLIANCE, OBJECT-GROUP,NOTIFICATION-GROUP
            FROM SNMPv2-CONF
        BITS, OBJECT-TYPE, MODULE-IDENTITY,NOTIFICATION-TYPE,Integer32
            FROM SNMPv2-SMI
        DateAndTime
            FROM SNMPv2-TC;


    --  Oct 25, 2005 at 19:00 GMT
    hwNetStreamMIB MODULE-IDENTITY 
        LAST-UPDATED "201507250000Z"
        ORGANIZATION 
            "Huawei Technologies Co.,Ltd."
        CONTACT-INFO 
            "Huawei Industrial Base
              Bantian, Longgang
               Shenzhen 518129
               People's Republic of China
               Website: http://www.huawei.com
               Email: support@huawei.com
             "
        DESCRIPTION 
            "The private mib file includes the general extent information of 
             the device.hwDatacomm(25).htNetStream(110)"
        REVISION "201507250000Z" 
        DESCRIPTION "Initial version"
        ::= { hwDatacomm 110 }


-- Top-level structure of the MIB
--1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1
hwNetStreamObjects             OBJECT IDENTIFIER ::= { hwNetStreamMIB 1 }
--1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 2
hwNetStreamNotifications       OBJECT IDENTIFIER ::= { hwNetStreamMIB 2 }

-- OBJECT IDENTIFIER definitions
    
    -- 1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1 , 1
    hwNetStreamlastchangedtime OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object is the time stamp, which describes the last time that
             the netStreamIfIndex table has been changed. "
        ::= { hwNetStreamObjects 1 }
    
    -- 1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1 , 2
    hwNetStreamIfIndexTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwNetStreamIfIndexEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This table contains tow rows, one of the two elements indicates 
             the interface index which is distributed by VRP, named 
             netStream32BitIndex and occupies 32 bits.Another indicates the
             interface index of netstream character, which named 
             netStream16BitIndex and occupies 16 bits."
        ::= { hwNetStreamObjects 2 }
    
    -- 1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1 , 2 , 1
    hwNetStreamIfIndexEntry OBJECT-TYPE
        SYNTAX HwNetStreamIfIndexEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Information about a replaceable unit physical entity. Each entry 
             provides objects of a replaceable unit to help an NMS identify 
             and characterize the entry in this table."
        INDEX { hwNetStream16BitIndex }
        ::= { hwNetStreamIfIndexTable 1 }
        
    HwNetStreamIfIndexEntry ::=
        SEQUENCE { 
            hwNetStream16BitIndex
                Integer32,
            hwifNet32BitIndex
                Integer32
         }

    -- 1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1 , 2 , 1 , 1
     hwNetStream16BitIndex OBJECT-TYPE
        SYNTAX Integer32 (0..65535)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "NetStream16BitIndex indicates the interface index of netstream character."
        ::= { hwNetStreamIfIndexEntry 1 }
    
    -- 1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1 , 2 , 1 , 2
   hwifNet32BitIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "NetStream32BitIndex indicates the interface index which is distributed by VRP."
        ::= { hwNetStreamIfIndexEntry 2 }
        
    -- 1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 1 , 3
    hwNetStreamTemplateRefresh OBJECT-TYPE
	SYNTAX Integer32 (1)
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"The object used to trigger netstream resend all templates."
	::= { hwNetStreamObjects 3 }
-- Type definitions
--1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 2 , 0
hwNetStreamTrapPrefix        OBJECT IDENTIFIER ::= { hwNetStreamNotifications 0 }

--1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 2 , 0 , 1
    hwNetStreamIndexStatusChanged NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION
            "The object indicates if the hwNetStreamIfIndexTable has been changed 
             when interface is deleted,created and board is inserted and drawed."
    ::= { hwNetStreamTrapPrefix 1 }
--1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 2 , 0 , 2
    hwNetStreamIndexUsedUp NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION
            "The object indicates if there is enough index to be distributed,
             which is on the managed object."

    ::= { hwNetStreamTrapPrefix 2 }
--1 , 3 , 6 , 1 , 4 , 1 , 2011 , 5 , 25 , 110 , 2 , 0 , 3
    hwNetStreamSessionFull NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION
            "The object indicates if the session is full."

    ::= { hwNetStreamTrapPrefix 3 }
    
-- conformance information 

   hwNetstreamConformance OBJECT IDENTIFIER ::= { hwNetStreamMIB 3 } 
   hwNetstreamGroups      OBJECT IDENTIFIER ::= { hwNetstreamConformance 1 }
   hwNetstreamCompliances  OBJECT IDENTIFIER ::= { hwNetstreamConformance 2 }
-- compliance statements

   hwNetstreamCompliance MODULE-COMPLIANCE
   STATUS  current
   DESCRIPTION
       "The compliance statement for SNMPv2 entities which implement the HUAWEI 
        Netstream extension MIB."
   MODULE  -- this module
   MANDATORY-GROUPS { hwNetstreamExtGroup ,hwNotificationExtGroup}
   ::= { hwNetstreamCompliances 1 }
-- units of conformance
hwNetstreamExtGroup OBJECT-GROUP
    OBJECTS {hwNetStreamlastchangedtime,hwNetStream16BitIndex, hwifNet32BitIndex,hwNetStreamTemplateRefresh}
    STATUS  current
    DESCRIPTION
       "The HUAWEI Netstream extension Table."
    ::= { hwNetstreamGroups 2 } 
hwNotificationExtGroup NOTIFICATION-GROUP
    NOTIFICATIONS { hwNetStreamIndexUsedUp, hwNetStreamIndexStatusChanged, hwNetStreamSessionFull }
    STATUS  current
    DESCRIPTION
        "The HUAWEI Netstream trap info."
    ::= { hwNetstreamGroups 3 }
END