
-- *****************************************************************************
-- Juniper-IP-TUNNEL-MIB
--
-- Juniper Networks Enterprise MIB
--   Extensions for IP Tunnel management
--
-- Copyright (c) 2001, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-IP-TUNNEL-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, IpAddress, Integer32
        FROM SNMPv2-SMI
    InterfaceIndex
        FROM IF-MIB
    RowStatus, DisplayString, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    JuniNextIfIndex, JuniName
        FROM Juniper-TC
    juniMibs
        FROM Juniper-MIBs;

juniIpTunnelMIB  MODULE-IDENTITY
    LAST-UPDATED "200309291729Z"  -- 29-Sep-03 01:29 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The IP Tunnel MIB for the Juniper Networks enterprise."
    -- Revision History
    REVISION    "200309291729Z"  -- 29-Sep-03 01:29 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "Product rebranding (JUNOSe)."
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200201141816Z"  -- 14-Jan-02 01:16 PM EST  - JUNOSe 4.1
    DESCRIPTION
        "Added juniIpTunnelSequenceNumbers."
    REVISION    "200107232057Z"  -- 23-Jul-01 04:57 PM EDT  - JUNOSe 3.2
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 51 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpTunnelInterfaceObjects    OBJECT IDENTIFIER ::= { juniIpTunnelMIB 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Tunnel Interface Objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- IfIndex selection for creating IP tunnel interfaces
--
juniIpTunnelNextIfIndex OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in juniIpTunnelIfTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniIpTunnelInterfaceObjects 1 }


--
-- The IP Tunnel Interface Table
--
juniIpTunnelInterfaceTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpTunnelInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries of IP Tunnel interfaces."
    ::= { juniIpTunnelInterfaceObjects 2 }

juniIpTunnelInterfaceEntry OBJECT-TYPE
    SYNTAX      JuniIpTunnelInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a single IP Tunnel
        interface.

        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/juniIfTable."
    INDEX     { juniIpTunnelIfIndex }
    ::= { juniIpTunnelInterfaceTable 1 }

JuniIpTunnelInterfaceEntry ::= SEQUENCE {
    juniIpTunnelIfIndex          InterfaceIndex,
    juniIpTunnelName             DisplayString,
    juniIpTunnelMode             INTEGER,
    juniIpTunnelVirtualRouter    JuniName,
    juniIpTunnelChecksum         TruthValue,
    juniIpTunnelMtu              Integer32,
    juniIpTunnelSource           IpAddress,
    juniIpTunnelDestination      IpAddress,
    juniIpTunnelRowStatus        RowStatus,
    juniIpTunnelSequenceNumbers  TruthValue }

juniIpTunnelIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the IP tunnel interface.  When creating entries in this
        table, suitable values for this object are determined by reading
        juniIpTunnelNextIfIndex."
    ::= { juniIpTunnelInterfaceEntry 1 }

juniIpTunnelName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..80))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administratively assigned name for this IP Tunnel interface."
    ::= { juniIpTunnelInterfaceEntry 2 }

juniIpTunnelMode OBJECT-TYPE
    SYNTAX      INTEGER {
                    ipTunnelModeGre(0),
                    ipTunnelModeDvmrp(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The configured mode for this IP Tunnel interface."
    ::= { juniIpTunnelInterfaceEntry 3 }

juniIpTunnelVirtualRouter OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The transport virtual router associated with this IP tunnel interface.
        This object need not be set when creating row entries.  Note that the
        default when this object is not specified is the router associated with
        the agent acting on the management request."
    DEFVAL    { "default" }
    ::= { juniIpTunnelInterfaceEntry 4 }

juniIpTunnelChecksum OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Tunnel checksum configuration for this entry.  Setting this object
        to true(1) will enabled end-to-end checksumming and will cause the
        system to drop packets with bad checksums received on this interface.
        Setting this object to false(2) will disable this feature.
        Note:  This configuration object is not supported for DVMRP tunnels."
    DEFVAL    { false }
    ::= { juniIpTunnelInterfaceEntry 5 }

juniIpTunnelMtu OBJECT-TYPE
    SYNTAX      Integer32 (1024..10240)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The tunnel MTU."
    DEFVAL    { 10240 }
    ::= { juniIpTunnelInterfaceEntry 6 }

juniIpTunnelDestination OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The tunnel destination IP address."
    DEFVAL    { 0 }
    ::= { juniIpTunnelInterfaceEntry 7 }

juniIpTunnelSource OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The tunnel source IP address."
    DEFVAL    { 0 }
    ::= { juniIpTunnelInterfaceEntry 8 }

juniIpTunnelRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpTunnelIfRowStatus
            juniIpTunnelName
            juniIpTunnelMode

        In addition, when creating an entry the following condition must hold:

            A value for juniIpTunnelIfIndex must have been determined
            previously, typically by reading juniIpTunnelNextIfIndex.

        Once created, the following objects may not be modified:
            juniIpTunnelName
            juniIpTunnelMode
            juniIpTunnelVirtualRouter

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table."
    ::= { juniIpTunnelInterfaceEntry 9 }

juniIpTunnelSequenceNumbers OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The tunnel sequence number configuration for this entry.  Setting this
        object to true(1) will enable sequence number generation.  Setting this
        object to false(2) will disable this feature.
        Note:  This configuration object is not supported for DVMRP tunnels."
    DEFVAL    { false }
    ::= { juniIpTunnelInterfaceEntry 10 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpTunnelConformance  OBJECT IDENTIFIER ::= { juniIpTunnelMIB 2 }
juniIpTunnelCompliances  OBJECT IDENTIFIER ::= { juniIpTunnelConformance 1 }
juniIpTunnelGroups       OBJECT IDENTIFIER ::= { juniIpTunnelConformance 2 }

--
-- compliance statements
--
juniIpTunnnelCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities that implement the Juniper
        IP Tunnel MIB.  This compliance statement became obsolete when
        juniIpTunnelSequenceNumbers was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpTunnelInterfaceGroup }
    ::= { juniIpTunnelCompliances 1 }                              -- JUNOSe 3.2

juniIpTunnnelCompliance2  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities that implement the Juniper IP
        Tunnel MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpTunnelInterfaceGroup2 }
    ::= { juniIpTunnelCompliances 2 }                              -- JUNOSe 4.1

--
-- units of conformance
--
juniIpTunnelInterfaceGroup  OBJECT-GROUP
    OBJECTS {
        juniIpTunnelNextIfIndex,
        juniIpTunnelName,
        juniIpTunnelMode,
        juniIpTunnelVirtualRouter,
        juniIpTunnelChecksum,
        juniIpTunnelMtu,
        juniIpTunnelSource,
        juniIpTunnelDestination,
        juniIpTunnelRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP Tunnel capabilities in a
        Juniper product.  This group became obsolete when
        juniIpTunnelSequenceNumbers was added."
    ::= { juniIpTunnelGroups 1 }                                   -- JUNOSe 3.2

juniIpTunnelInterfaceGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpTunnelNextIfIndex,
        juniIpTunnelName,
        juniIpTunnelMode,
        juniIpTunnelVirtualRouter,
        juniIpTunnelChecksum,
        juniIpTunnelMtu,
        juniIpTunnelSource,
        juniIpTunnelDestination,
        juniIpTunnelRowStatus,
        juniIpTunnelSequenceNumbers }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP Tunnel capabilities in a
        Juniper product."
    ::= { juniIpTunnelGroups 2 }                                   -- JUNOSe 4.1

END
