--MibName=raisecomSystem
-- =======================================================================
-- Version info
--
-- Version 0.1 Created 2003.12.17 by GONGGUIDONG
-- This version of MIB is created just for the use of Network Management Systems
-- display the  memory and cpu.
--
-- Copyright(c) 2002-2005 by RAISECOM TECH, Ltd.
-- modify history
-- 01, 20131012, huxiangfeng, Add two traps.
-- 01, 20090915, qiyun, Add CPU monitor MIBs.
--
-- =======================================================================



ROSMGMT-SYSTEM-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY ,
        NOTIFICATION-TYPE,
        Integer32,
        OBJECT-TYPE
                    FROM SNMPv2-SMI
        rosMgmt
                    FROM RAISECOM-BASE-MIB

        EnableVar
                    FROM SWITCH-TC
        TimeStamp,TEXTUAL-CONVENTION
                    FROM SNMPv2-TC;

    rosMgmtSystem MODULE-IDENTITY
                LAST-UPDATED     "202004120000Z"
                ORGANIZATION     "RAISECOM TECH, Ltd."
                CONTACT-INFO     "www.raisecom.com"
                DESCRIPTION
                        "raisecom System objects: objects common to all platforms."
        REVISION        "202004120000Z"
        DESCRIPTION     "MIB file check and modification"
            ::= { rosMgmt 1 }
--
-- Textual Conventions
--

    ProcessStatus ::= TEXTUAL-CONVENTION
        STATUS    current
        DESCRIPTION
                   "Status of the process."
        SYNTAX   INTEGER
                {
                rrunning(1),
                dinterruptiblesleep(2),
                suninterruptiblesleep(3),
                tstopped(4),
                zzombie(5),
                xdead(6),
                wpaging(7)
                }

    CPUTimeStamp ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "4d.4d.4d.4d"
        STATUS       current
        DESCRIPTION
                "The time in seconds that could represent signed
                quantities like time delay with respect to some
                source. The signed integer part is in the first
                32 bits and the fraction part is in the last 32 bits."
        REFERENCE
                "D.L. Mills, 'Network Time Protocol (Version 3)',
                RFC-1305, March 1992, Sections 2,  3.2.1"
        SYNTAX     OCTET STRING (SIZE (16))


--
-- RAISECOM CPU objects
--


    rosMgmtCpu    OBJECT IDENTIFIER ::= { rosMgmtSystem 1 }

--rosMgmtCpuTrapGroup

    rosMgmtCpuNotifications    OBJECT IDENTIFIER ::= { rosMgmtCpu 0 }
    rosMgmtCpuObjects          OBJECT IDENTIFIER ::= { rosMgmtCpu 1 }
    rosMgmtCpuConformance      OBJECT IDENTIFIER ::= { rosMgmtCpu 2 }

--rosMgmtCpuNotifications
     rosMgmtCpuRisingThreshold NOTIFICATION-TYPE
            OBJECTS { rosMgmtProcessIndex, rosMgmtProcessUtilization,rosMgmtCpuUtilizationCpuIdx, rosMgmtCpuUtilization }
            STATUS  current
            DESCRIPTION
                 "CPU utilization rising threshold trap transfer."
            ::= { rosMgmtCpuNotifications 1 }

     rosMgmtCpuRisingThresholdRecover NOTIFICATION-TYPE
            OBJECTS {rosMgmtCpuUtilizationCpuIdx, rosMgmtCpuUtilization }
            STATUS  current
            DESCRIPTION
                 "CPU utilization rising threshold return to normal trap transfer."
            ::= { rosMgmtCpuNotifications 2 }


--rosMgmtCpuScalarGroup


       rosMgmtCpuScalarGroup  OBJECT IDENTIFIER
                   ::= { rosMgmtCpuObjects 1}

        rosMgmtCpuTotalProcNum OBJECT-TYPE
                   SYNTAX  Integer32   (1..2000)
                   MAX-ACCESS  read-only
                   STATUS  current
                   DESCRIPTION
                          "Total number of processes."
                   ::= { rosMgmtCpuScalarGroup 1}


       rosMgmtCpuHistoryTableSize OBJECT-TYPE
                   SYNTAX  Integer32
                   MAX-ACCESS  read-only
                   STATUS  current
                   DESCRIPTION
                          "A value configured by the user which specifies
                          the number of reports in the history table."
                   DEFVAL { 60 }
                   ::= { rosMgmtCpuScalarGroup 2}

       rosMgmtCpuThresholdTrapEnable OBJECT-TYPE
                   SYNTAX  EnableVar
                   MAX-ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                          "The administration status of the CPU utilization threshold trap."
                   ::= { rosMgmtCpuScalarGroup 3}

       rosMgmtCpuRisingThresholdValue OBJECT-TYPE
                   SYNTAX  Integer32  (2..99)
                   MAX-ACCESS  read-write
                   STATUS  current
                   DESCRIPTION
                          "The percentage rising threshold value configured by the user.
                          The value indicates, if the CPU utilization which rise from
                          rosMgmtCpuFallingThresholdValue is equal to or above this value
                          for rosMgmtCpuThresholdInterval duration then send
                          a rosMgmtCpuRisingThreshold notification to the NMS."
                   DEFVAL { 99 }
                   ::= { rosMgmtCpuScalarGroup 4}

       rosMgmtCpuRecoverThresholdValue OBJECT-TYPE
                   SYNTAX  Integer32  (0..98)
                   MAX-ACCESS  read-write
                   STATUS  current
                   DESCRIPTION
                          "The percentage falling threshold value configured by the user.
                          The value indicates, if the CPU utilization which fell from
                          rosMgmtCpuRecoverThresholdValue is equal to or below this value
                          for rosMgmtCpuThresholdInterval duration then send
                          a rosMgmtCpuFallingThreshold notification to the NMS."
                   DEFVAL { 79 }
                   ::= { rosMgmtCpuScalarGroup 5}

       rosMgmtCpuThresholdInterval OBJECT-TYPE
                   SYNTAX  Integer32  (5..36000)
                   MAX-ACCESS  read-write
                   STATUS  current
                   DESCRIPTION
                          "This is an observation interval.
                          The value of this object indicates that the CPU utilization
                          should be above rosMgmtCpuRisingThresholdValue for this
                          duration to send a rosMgmtCpuRisingThreshold notification
                          to the NMS or below rosMgmtCpuFallingThresholdValue for
                          this duration to send a rosMgmtCpuFallingThreshold."
                   DEFVAL { 60 }
                   ::= { rosMgmtCpuScalarGroup 6}

        rosMgmtCpuNum OBJECT-TYPE
                   SYNTAX  Integer32
                   MAX-ACCESS  read-only
                   STATUS  current
                   DESCRIPTION
                          "Total number of cpu."
                   ::= { rosMgmtCpuScalarGroup 7}



--rosMgmtCpuTableGroup


       rosMgmtCpuTableGroup  OBJECT IDENTIFIER
                   ::= { rosMgmtCpuObjects 2}


--rosMgmtCpuUtilizationGroup


       rosMgmtCpuUtilizationGroup  OBJECT IDENTIFIER
                   ::= { rosMgmtCpuTableGroup 1 }


--rosMgmtCpuUtilizationTable

       rosMgmtCpuUtilizationTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF RosMgmtCpuUtilizationEntry
                   MAX-ACCESS  not-accessible
                   STATUS  current
                   DESCRIPTION
                            "This table contains information about multi-core CPU utilization."
                   ::= { rosMgmtCpuUtilizationGroup 1 }

       rosMgmtCpuUtilizationEntry OBJECT-TYPE
                    SYNTAX  RosMgmtCpuUtilizationEntry
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                            "Information about the CPU utilization."
                    INDEX           { rosMgmtCpuUtilizationPeriod,rosMgmtCpuUtilizationCpuIdx }
                    ::= { rosMgmtCpuUtilizationTable 1 }

       RosMgmtCpuUtilizationEntry ::= SEQUENCE {
                    rosMgmtCpuUtilizationPeriod    INTEGER,
                    rosMgmtCpuUtilizationCpuIdx    Integer32,
                    rosMgmtCpuUtilization          Integer32
                    }

       rosMgmtCpuUtilizationPeriod OBJECT-TYPE
                    SYNTAX    INTEGER {
                                        oneSec(1),
                                        fiveSec(2),
                                        oneMin(3),
                                        tenMin(4),
                                        twoHour(5)
                                    }
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Periods for computing CPU utilization."
                    ::= { rosMgmtCpuUtilizationEntry 1 }

       rosMgmtCpuUtilizationCpuIdx OBJECT-TYPE
                    SYNTAX Integer32 (0..16)
                    MAX-ACCESS read-only
                    STATUS current
                    DESCRIPTION
                        "The cpu core index"
                    ::= { rosMgmtCpuUtilizationEntry 2 }


       rosMgmtCpuUtilization OBJECT-TYPE
                    SYNTAX  Integer32
                    UNITS    "percent"
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "CPU busy percentage in the last specified period."
                    ::= { rosMgmtCpuUtilizationEntry 3 }

--rosMgmtTotalCPUUtilizationTable


       rosMgmtTotalCPUUtilizationTable OBJECT-TYPE
                    SYNTAX SEQUENCE OF RosMgmtTotalCPUUtilizationEntry
                    MAX-ACCESS not-accessible
                    STATUS current
                    DESCRIPTION
                        "This table contains information about total CPU utilization."
                    ::= { rosMgmtCpuUtilizationGroup 2 }

        rosMgmtTotalCPUUtilizationEntry OBJECT-TYPE
                    SYNTAX RosMgmtTotalCPUUtilizationEntry
                    MAX-ACCESS not-accessible
                    STATUS current
                    DESCRIPTION
                        "Description."
                    INDEX { rosMgmtTotalCPUPeriod }
                    ::= { rosMgmtTotalCPUUtilizationTable 1 }

        RosMgmtTotalCPUUtilizationEntry ::= SEQUENCE {
                    rosMgmtTotalCPUPeriod          INTEGER,
                    rosMgmtTotalCPUUtilization     Integer32
                    }

        rosMgmtTotalCPUPeriod OBJECT-TYPE
                    SYNTAX INTEGER  {
                                        oneSec(1),
                                        fiveSec(2),
                                        oneMin(3),
                                        tenMin(4),
                                        twoHour(5)
                                    }
                    MAX-ACCESS not-accessible
                    STATUS current
                    DESCRIPTION
                        "Periods for computing CPU utilization."
                    ::= { rosMgmtTotalCPUUtilizationEntry 1 }


        rosMgmtTotalCPUUtilization OBJECT-TYPE
                    SYNTAX Integer32 (0..10000)
                    UNITS "percent"
                    MAX-ACCESS read-only
                    STATUS current
                    DESCRIPTION
                        "CPU busy percentage in the last specified period."
                    ::= { rosMgmtTotalCPUUtilizationEntry 2 }




--rosMgmtCpuHistoryTable

       rosMgmtCpuHistoryTable OBJECT-TYPE
                   SYNTAX   SEQUENCE OF RosMgmtCpuHistoryEntry
                   MAX-ACCESS   not-accessible
                   STATUS   current
                   DESCRIPTION
                            "This table contains CPU hsitory utilization records."
                   ::= { rosMgmtCpuUtilizationGroup 3}

       rosMgmtCpuHistoryEntry OBJECT-TYPE
                    SYNTAX  RosMgmtCpuHistoryEntry
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                            "CPU history utilization record."
                    INDEX           { rosMgmtCpuHistoryPeriod, rosMgmtCpuHistoryIndex,rosMgmtCpuHistoryCpuIdx }
                    ::= { rosMgmtCpuHistoryTable 1 }

       RosMgmtCpuHistoryEntry ::= SEQUENCE {
                       rosMgmtCpuHistoryPeriod     INTEGER,
                    rosMgmtCpuHistoryIndex      Integer32,
                    rosMgmtCpuHistoryCpuIdx     Integer32,
                    rosMgmtCpuHistoryUtil  Integer32
                    }

       rosMgmtCpuHistoryPeriod OBJECT-TYPE
                    SYNTAX    INTEGER {
                                        fiveSec(1),
                                        oneMin(2),
                                        tenMin(3),
                                        twoHour(4)
                                    }
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Periods for computing CPU history utilization, the first index of CPU history utilization table."
                    ::= { rosMgmtCpuHistoryEntry 1 }

       rosMgmtCpuHistoryIndex OBJECT-TYPE
                    SYNTAX    Integer32   (1..60)
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Process sequence number,the second index of CPU history utilization table."
                    ::= { rosMgmtCpuHistoryEntry 2 }

       rosMgmtCpuHistoryCpuIdx OBJECT-TYPE
                    SYNTAX Integer32 (0..16)
                    MAX-ACCESS read-only
                    STATUS current
                    DESCRIPTION
                        "The cpu core index"
                    ::= { rosMgmtCpuHistoryEntry 3 }

       rosMgmtCpuHistoryUtil OBJECT-TYPE
                    SYNTAX    Integer32
                    UNITS    "percent"
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "History record of CPU utilization in the specified period. "
                    ::= { rosMgmtCpuHistoryEntry 4 }

--rosMgmtTotalCPUHistoryTable

       rosMgmtTotalCPUHistoryTable OBJECT-TYPE
                   SYNTAX   SEQUENCE OF RosMgmtTotalCPUHistoryEntry
                   MAX-ACCESS   not-accessible
                   STATUS   current
                   DESCRIPTION
                            "This table contains CPU hsitory utilization records."
                   ::= { rosMgmtCpuUtilizationGroup 4}

       rosMgmtTotalCPUHistoryEntry OBJECT-TYPE
                    SYNTAX  RosMgmtTotalCPUHistoryEntry
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                            "CPU history utilization record."
                    INDEX           { rosMgmtTotalCPUHistoryPeriod, rosMgmtTotalCPUHistoryIndex }
                    ::= { rosMgmtTotalCPUHistoryTable 1 }

       RosMgmtTotalCPUHistoryEntry ::= SEQUENCE {
                       rosMgmtTotalCPUHistoryPeriod     INTEGER,
                    rosMgmtTotalCPUHistoryIndex      Integer32,
                    rosMgmtTotalCPUHistoryUtil  Integer32
                    }

       rosMgmtTotalCPUHistoryPeriod OBJECT-TYPE
                    SYNTAX    INTEGER {
                                        fiveSec(1),
                                        oneMin(2),
                                        tenMin(3),
                                        twoHour(4)
                                    }
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Periods for computing CPU history utilization, the first index of CPU history utilization table."
                    ::= { rosMgmtTotalCPUHistoryEntry 1 }

       rosMgmtTotalCPUHistoryIndex OBJECT-TYPE
                    SYNTAX    Integer32  (1..60)
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Process sequence number,the second index of CPU history utilization table."
                    ::= { rosMgmtTotalCPUHistoryEntry 2 }

       rosMgmtTotalCPUHistoryUtil OBJECT-TYPE
                    SYNTAX    Integer32
                    UNITS    "percent"
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "History record of CPU utilization in the specified period. "
                    ::= { rosMgmtTotalCPUHistoryEntry 3 }


--rosMgmtCpuProcessesGroup


       rosMgmtCpuProcessesGroup  OBJECT IDENTIFIER
                   ::= { rosMgmtCpuTableGroup 2 }


--rosMgmtProcessesTable

       rosMgmtProcessesTable OBJECT-TYPE
                   SYNTAX   SEQUENCE OF RosMgmtProcessesEntry
                   MAX-ACCESS   not-accessible
                   STATUS   current
                   DESCRIPTION
                            "This table contains information about processes."
                   ::= { rosMgmtCpuProcessesGroup 1 }

       rosMgmtProcessesEntry OBJECT-TYPE
                    SYNTAX  RosMgmtProcessesEntry
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                            "Information about processes."
                    INDEX           { rosMgmtProcessIndex }
                    ::= { rosMgmtProcessesTable 1 }

       RosMgmtProcessesEntry ::= SEQUENCE {
                    rosMgmtProcessIndex            Integer32,
                    rosMgmtProcessPID              Integer32,
                    rosMgmtProcessName             OCTET STRING,
                    rosMgmtProcessRunTimeTotal     CPUTimeStamp,
                    rosMgmtProcessInvokedTotal        Integer32,
                    rosMgmtProcessTimeCreated      TimeStamp,
                    rosMgmtProcessCurrentPriority  Integer32,
                    rosMgmtProcessStatus           ProcessStatus
                    }

       rosMgmtProcessIndex OBJECT-TYPE
                    SYNTAX  Integer32   (1..2147483647)
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "This object index of processes table. This index is PID."
                    ::= { rosMgmtProcessesEntry 1 }

       rosMgmtProcessPID OBJECT-TYPE
                    SYNTAX  Integer32
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "This object contains the process ID."
                    ::= { rosMgmtProcessesEntry 2 }

       rosMgmtProcessName OBJECT-TYPE
                    SYNTAX  OCTET STRING (SIZE(1..32))
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The name associated with this process."
                    ::= { rosMgmtProcessesEntry 3 }

       rosMgmtProcessRunTimeTotal OBJECT-TYPE
                    SYNTAX  CPUTimeStamp
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The amount of time the process occupied, in microseconds."
                    ::= { rosMgmtProcessesEntry 4 }

       rosMgmtProcessInvokedTotal OBJECT-TYPE
                    SYNTAX  Integer32
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The number of times since rosMgmtProcessTimeCreated
                    that the process has been invoked."
                    ::= { rosMgmtProcessesEntry 5 }

       rosMgmtProcessTimeCreated OBJECT-TYPE
                    SYNTAX  TimeStamp
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The time when the process was created.
                    The process sequence number and the time
                    when the process was created, uniquely identifies a process."
                    ::= { rosMgmtProcessesEntry 6 }

       rosMgmtProcessCurrentPriority OBJECT-TYPE
                    SYNTAX  Integer32
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The current priority at which the process is running."
                    ::= { rosMgmtProcessesEntry 7 }

       rosMgmtProcessStatus OBJECT-TYPE
                    SYNTAX  ProcessStatus
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The current status of the process."
                    ::= { rosMgmtProcessesEntry 8 }



--rosMgmtProcessStatisticsTable

       rosMgmtProcessStatisticsTable OBJECT-TYPE
                   SYNTAX   SEQUENCE OF RosMgmtProcessStatisticsEntry
                   MAX-ACCESS   not-accessible
                   STATUS   current
                   DESCRIPTION
                            "This table contains statistics information for processes.
                            The first index is rosMgmtProcessIndex,
                            the second index is rosMgmtProcessStatisticsPeriod"
                   ::= { rosMgmtCpuProcessesGroup 2 }

       rosMgmtProcessStatisticsEntry OBJECT-TYPE
                    SYNTAX  RosMgmtProcessStatisticsEntry
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                            "Statistics information for processes."
                    INDEX           { rosMgmtProcessIndex, rosMgmtProcessStatisticsPeriod }
                    ::= { rosMgmtProcessStatisticsTable 1 }

       RosMgmtProcessStatisticsEntry ::= SEQUENCE {
                    rosMgmtProcessStatisticsPeriod    INTEGER,
                    rosMgmtProcessRunTime             CPUTimeStamp,
                    rosMgmtProcessUtilization         Integer32
                    }

       rosMgmtProcessStatisticsPeriod OBJECT-TYPE
                    SYNTAX    INTEGER {
                                        fiveSec(1),
                                        oneMin(2),
                                        tenMin(3)
                                    }
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Periods for process statistics,
                    the second index of process statistics table."
                    ::= { rosMgmtProcessStatisticsEntry 1 }

       rosMgmtProcessRunTime OBJECT-TYPE
                    SYNTAX    CPUTimeStamp
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "Time of the process occupied in the specified period."
                    ::= { rosMgmtProcessStatisticsEntry 2 }

       rosMgmtProcessUtilization OBJECT-TYPE
                    SYNTAX    Integer32
                    UNITS    "percent"
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "This object provides a general idea of how busy
                    a process caused the processor to be over a specified period."
                    ::= { rosMgmtProcessStatisticsEntry 3 }


--rosMgmtDeadProcessesTable

       rosMgmtDeadProcessesTable OBJECT-TYPE
                   SYNTAX   SEQUENCE OF RosMgmtDeadProcessesEntry
                   MAX-ACCESS   not-accessible
                   STATUS   current
                   DESCRIPTION
                            "This table contains dead processes information."
                   ::= { rosMgmtCpuProcessesGroup 3 }

       rosMgmtDeadProcessesEntry OBJECT-TYPE
                    SYNTAX  RosMgmtDeadProcessesEntry
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                            "Dead processes information."
                    INDEX           { rosMgmtDeadProcessIndex }
                    ::= { rosMgmtDeadProcessesTable 1 }

       RosMgmtDeadProcessesEntry ::= SEQUENCE {
                    rosMgmtDeadProcessIndex        Integer32 ,
                    rosMgmtDeadProcessName         OCTET STRING,
                    rosMgmtDeadProcessPriority     Integer32,
                    rosMgmtDeadProcessTimeDelete   TimeStamp,
                    rosMgmtDeadProcessDeadTimes    Integer32,
                    rosMgmtDeadProcessStatus       ProcessStatus
                    }

       rosMgmtDeadProcessIndex OBJECT-TYPE
                    SYNTAX    Integer32   (1..2147483647)
                    MAX-ACCESS  not-accessible
                    STATUS  current
                    DESCRIPTION
                    "Process sequence number,the index of dead processes table. The index is PID."
                    ::= { rosMgmtDeadProcessesEntry 1 }

       rosMgmtDeadProcessName OBJECT-TYPE
                    SYNTAX    OCTET STRING (SIZE(1..32))
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The name associated with this dead process."
                    ::= { rosMgmtDeadProcessesEntry 2 }

       rosMgmtDeadProcessPriority OBJECT-TYPE
                    SYNTAX    Integer32
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The priority at which the dead process."
                    ::= { rosMgmtDeadProcessesEntry 3 }


       rosMgmtDeadProcessTimeDelete OBJECT-TYPE
                    SYNTAX    TimeStamp
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The time when the process was deleted."
                    ::= { rosMgmtDeadProcessesEntry 4}

       rosMgmtDeadProcessDeadTimes OBJECT-TYPE
                    SYNTAX    Integer32
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "Times of the process dead."
                    ::= { rosMgmtDeadProcessesEntry 5 }

       rosMgmtDeadProcessStatus OBJECT-TYPE
                    SYNTAX    ProcessStatus
                    MAX-ACCESS  read-only
                    STATUS  current
                    DESCRIPTION
                    "The status of the dead process."
                    ::= { rosMgmtDeadProcessesEntry 6}



END