--
-- ALARM-MIB.my
-- MIB generated by MG-SOFT Visual MIB Builder Version 4.0 Build 349
-- Friday, November 21, 2003 at 15:00:38
--



	SPIDCOM-TRAPS DEFINITIONS ::= BEGIN

		IMPORTS
			OBJECT-GROUP, NOTIFICATION-GROUP
				FROM SNMPv2-CONF
			Integer32, Unsigned32, Counter32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE
				FROM SNMPv2-SMI
			specificSpidcomTrap
				FROM SPIDCOM-NOTIFICATION-MIB
			ItuAlarmProbableCause,ItuAlarmType, neAlarmActivePhoto
				FROM SPIDCOM-ALARM-MIB
			plcBasePortIndex
				FROM SPC200
			DisplayString, DateAndTime, TEXTUAL-CONVENTION
				FROM SNMPv2-TC;



--
-- Node definitions
--

		-- 1.3.6.1.4.1.22764.4.1
		trapsDefinition MODULE-IDENTITY
			LAST-UPDATED "200207151330Z"		-- July 15, 2002 at 13:30 GMT
			ORGANIZATION
				"SPiDCOM"

			CONTACT-INFO
				" TO BE SPECIFIED BY SPiDCOM
				"
			DESCRIPTION
				"Definition of the MIB tree structure
				to manage the Alarm Monitoring."
			::= { specificSpidcomTrap 1 }



		-- 1.3.6.1.4.1.22764.4.1.1
		deviceDown NOTIFICATION-TYPE
			STATUS current
			DESCRIPTION
				"This trap is sent when a the connection with a distant node is down"
			::= { trapsDefinition 1 }


		-- 1.3.6.1.4.1.22764.4.1.2
		deviceUp NOTIFICATION-TYPE
			STATUS current
			DESCRIPTION
				"This trap is sent when a the connection with a distant node is down"
			::= { trapsDefinition 2 }

		-- 1.3.6.1.4.1.22764.4.1.3
		maxAttenuation NOTIFICATION-TYPE
			STATUS current
			DESCRIPTION
				"This trap is sent when some value is reached for attenuation"
			::= { trapsDefinition 3 }

		-- 1.3.6.1.4.1.22764.4.1.4
		maxNoise NOTIFICATION-TYPE
			STATUS current
			DESCRIPTION
				"This trap is sent when some value is reached for noise"
			::= { trapsDefinition 4 }

		-- 1.3.6.1.4.1.22764.4.1.11
		linkUpDownNotificationsGroup NOTIFICATION-GROUP
			NOTIFICATIONS {
				deviceUp,
				deviceDown }
			STATUS current
			DESCRIPTION
				"The notifications which indicates connection with a distant node is up/down"
			::= { trapsDefinition 11 }

		-- 1.3.6.1.4.1.22764.4.1.12
		maxAttenuationNotificationsGroup NOTIFICATION-GROUP
			NOTIFICATIONS {
				maxAttenuation }
			STATUS current
			DESCRIPTION
				"The notification which indicates attenuation change"
			::= { trapsDefinition 12 }

		-- 1.3.6.1.4.1.22764.4.1.13
		maxNoiseNotificationsGroup NOTIFICATION-GROUP
			NOTIFICATIONS {
				maxNoise }
			STATUS current
			DESCRIPTION
				"The notification which indicates noise change"
			::= { trapsDefinition 13 }






	END

--
-- SPIDCOM-NOTIFICATION-MIB.my
--
