-- This module defines enterprise MIBs for email notification
-- setting
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-SET-EMAIL-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenSetting, netscreenSettingMibModule
        FROM NETSCREEN-SMI
    MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenSetEmailMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are used to monitor 
         the email notification setting"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311100000Z" -- November 10, 2003
    DESCRIPTION
        "Correct wrong title"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "No Comment"
    REVISION      "200105270000Z" -- May 27, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenSettingMibModule 7 }

nsSetEmail OBJECT IDENTIFIER ::= { netscreenSetting 7 }

nsSetEmailEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Enable E-mail Notification for Alarms"
    ::= { nsSetEmail 1 }

nsSetEmailSMTP OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SMTP server name"
    ::= { nsSetEmail 2 }

nsSetEmailLog OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Include Traffic Log in email"
    ::= { nsSetEmail 3 }

nsSetEmailAddr1 OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..64))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "E-mail receiver address one"
    ::= { nsSetEmail 4 }

nsSetEmailAddr2 OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..64))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "E-mail receiver address two"
    ::= { nsSetEmail 5 }

END


