-- *****************************************************************
-- Meru Networks Enterprise Specific MIB
--
-- Copyright (c) 2005 by Meru Networks
-- All rights reserved
--
-- *****************************************************************

MERU-CONFIG-SNMP-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    NOTIFICATION-TYPE, 
    OBJECT-TYPE, 
    MODULE-IDENTITY, 
    OBJECT-IDENTITY,
    enterprises, 
    Counter32, 
    Counter64, 
    Gauge32, 
    TimeTicks, 
    IpAddress, 
    Integer32
        FROM SNMPv2-SMI
    Ipv6Address
        FROM IPV6-TC
    TEXTUAL-CONVENTION, 
    TimeInterval, 
    TimeStamp,
    DateAndTime, 
    TruthValue, 
    DisplayString, 
    MacAddress, 
    RowStatus
        FROM SNMPv2-TC
    mwConfiguration
        FROM MERU-SMI
    ;

  mwConfigSnmp  MODULE-IDENTITY
    LAST-UPDATED "200506050000Z"
    ORGANIZATION "Meru Networks"
    CONTACT-INFO "support@merunetworks.com"
    DESCRIPTION
        "This MIB defines all the managed objects used to manage the Meru WLAN 
         SNMP Configuration infrastructure"
    ::= { mwConfiguration 12 } 
  
    
  
  mwWncTrapCommunityTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwWncTrapCommunityEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes SNMP Trap Management "
    ::= { mwConfigSnmp 2 }

  mwWncTrapCommunityEntry  OBJECT-TYPE
    SYNTAX MwWncTrapCommunityEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes SNMP Trap Management "
    INDEX {  mwWncTrapCommunityTableIndex  }
    ::= { mwWncTrapCommunityTable 1 }

  MwWncTrapCommunityEntry  ::=  SEQUENCE { 
       mwWncTrapCommunityTableIndex                                Integer32, 
       mwWncTrapCommunitypCommunityStr                             DisplayString(SIZE (1..32)),
       mwWncTrapCommunityClientIpAddress                           IpAddress,
       mwWncTrapCommunityRowStatus                                 RowStatus 
  }
   
   
  mwWncTrapCommunityTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwWncTrapCommunityEntry 1 }

  mwWncTrapCommunitypCommunityStr  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (1..32))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Trap Community"
    ::= { mwWncTrapCommunityEntry    2 }

  mwWncTrapCommunityClientIpAddress  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Trap Destination IP"
    ::= { mwWncTrapCommunityEntry    3 }

  mwWncTrapCommunityRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwWncTrapCommunityEntry 4 }

  
END
   