-- *****************************************************************
-- Meru Networks Enterprise Specific MIB
--
-- Copyright (c) 2005 by Meru Networks
-- All rights reserved
--
-- *****************************************************************

MERU-CONFIG-GRE-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    NOTIFICATION-TYPE, 
    OBJECT-TYPE, 
    MODULE-IDENTITY, 
    OBJECT-IDENTITY,
    enterprises, 
    Counter32, 
    Counter64, 
    Gauge32, 
    TimeTicks, 
    IpAddress, 
    Integer32
        FROM SNMPv2-SMI
    Ipv6Address
        FROM IPV6-TC
    TEXTUAL-CONVENTION, 
    TimeInterval, 
    TimeStamp,
    DateAndTime, 
    TruthValue, 
    DisplayString, 
    MacAddress, 
    RowStatus
        FROM SNMPv2-TC
    mwConfiguration
        FROM MERU-SMI
    MwlOnOffSwitch,
    MwlProfileOwner
        FROM MERU-TC;

  mwConfigGRE  MODULE-IDENTITY
    LAST-UPDATED "200506050000Z"
    ORGANIZATION "Meru Networks"
    CONTACT-INFO "support@merunetworks.com"
    DESCRIPTION
        "This MIB defines all the managed objects used to manage the Meru WLAN 
         GRE Configuration infrastructure"
    ::= { mwConfiguration 15 } 
  
    
  
  mwGreTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF MwGreEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes GRE Configuration "
    ::= { mwConfigGRE 1 }

  mwGreEntry  OBJECT-TYPE
    SYNTAX MwGreEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
         "This object describes GRE Configuration "
    INDEX {  mwGreTableIndex  }
    ::= { mwGreTable 1 }

  MwGreEntry  ::=  SEQUENCE { 
       mwGreTableIndex                                             Integer32, 
       mwGreName                                                   DisplayString(SIZE (1..32)),
       mwGreInterfaceIndex                                         Unsigned32,
       mwGreDHCPServerIpAddress                                    IpAddress,
       mwGreLocalInternalAddress                                   IpAddress,
       mwGreLocalInternalNetmask                                   IpAddress,
       mwGreRemoteEndpointAddress                                  IpAddress,
       mwGreOverrideDefaultDHCPServer                              MwlOnOffSwitch,
       mwGreOwner                                                  MwlProfileOwner,
       mwGreRowStatus                                              RowStatus 
  }
   
   
  mwGreTableIndex  OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
         "The index value of the  table "
    ::= { mwGreEntry 1 }

  mwGreName  OBJECT-TYPE
    SYNTAX DisplayString(SIZE (1..32))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes GRE Name"
    ::= { mwGreEntry    2 }

  mwGreInterfaceIndex  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Local External Ethernet Index"
    ::= { mwGreEntry    3 }

  mwGreDHCPServerIpAddress  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes DHCP Server IP Address"
    ::= { mwGreEntry    4 }

  mwGreLocalInternalAddress  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Tunnel IP address"
    ::= { mwGreEntry    5 }

  mwGreLocalInternalNetmask  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Tunnel IP Netmask"
    ::= { mwGreEntry    6 }

  mwGreRemoteEndpointAddress  OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Remote External Address"
    ::= { mwGreEntry    7 }

  mwGreOverrideDefaultDHCPServer  OBJECT-TYPE
    SYNTAX MwlOnOffSwitch
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object describes Override Default DHCP Server Flag"
    ::= { mwGreEntry    8 }

  mwGreOwner  OBJECT-TYPE
    SYNTAX MwlProfileOwner
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "This object describes Owner"
    ::= { mwGreEntry    9 }

  mwGreRowStatus  OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
         "This object is used to create and delete rows in the table"
    ::= { mwGreEntry 17 }

  
END
   